The purpose of this model is to have the ability to log history data from channel when in demand.

For example, we want to record 1 millisecond of Volt activity before spike and 2 milliseconds after.

10 delayed channels

Record Trigger

Delayed Buffer to Log Model

10 Input channels